Product Carbon Footprint Report for vistydftvv

carboncalcpcf.com

Product Carbon Footprint Analysis Report

Product: vistydftvv

Company Name: sfugvuouri

Protocol Data (Accounting Standard): GHG Protocol

Senior Sustainability Consultant: mvvknuhzvk

Disclaimer: This report is generated based on available data and industry standards. While every effort has been made to ensure accuracy and adherence to the specified methodologies, the results are indicative and subject to the completeness and quality of the input data and chosen emission factors.

Product Carbon Footprint Analysis Report: vistydftvv

Generated Date: May 28, 2026

Prepared for: sfugvuouri

Prepared by: mvvknuhzvk, Senior Sustainability Consultant

Executive Summary

This report presents a high-detail Product Carbon Footprint (PCF) analysis for the product "vistydftvv" manufactured by "sfugvuouri". The assessment was conducted by Senior Sustainability Consultant mvvknuhzvk, adhering strictly to the Greenhouse Gas (GHG) Protocol, including the 2026 Land Sector and Removals (LSR) Standard update and the 95% Scope 3 coverage requirement. The analysis covers the entire lifecycle of vistydftvv, from raw material extraction and processing to its end-of-life, within a "factory_gate" system boundary for direct operational control and a broader "cradle-to-grave" approach for value chain impacts. Key insights into emission hotspots across the product\'s lifecycle are provided, alongside recommendations for reduction.

Methodology and Scope Definition

1. Define Scope

Functional Unit: The functional unit for this PCF analysis is 1.0 unit of vistydftvv.

System Boundary: The system boundary is defined as "factory_gate" for direct operational control. However, in line with GHG Protocol\'s comprehensive Scope 3 requirements, the analysis effectively extends to a "cradle-to-grave" perspective for all indirect value chain emissions. This includes raw material acquisition, manufacturing, transport, product use, and end-of-life treatment.

Geographic Scope:

Final Production Country: China

Supply Chain Focus: Europe Focused (for raw material sourcing and distribution to end-users in Europe)

Accounting Standard: This analysis rigorously follows the GHG Protocol standards for corporate value chain (Scope 3) accounting and reporting. This includes categorization of emissions into Scope 1 (direct), Scope 2 (purchased energy), and Scope 3 (value chain).

Allocation: Emissions are allocated directly to the functional unit (1.0 unit of vistydftvv) based on material quantities, energy consumption, and transport activities attributable to this unit. Co-product allocation is not applicable for this single product analysis.

Adherence to GHG Protocol and 2026 Updates:

GHG Protocol Categorization: Emissions are categorized into Scope 1 (direct emissions from owned/controlled sources), Scope 2 (indirect emissions from purchased energy), and Scope 3 (all other indirect emissions across the value chain).

2026 LSR Update: The Land Sector and Removals (LSR) Standard, effective January 1, 2027, has been considered. While specific land-use change data for materials is not explicitly provided, the principles of accounting for land-based emissions and carbon removals are acknowledged. The LSR Standard provides requirements for corporate GHG accounting covering emissions and carbon removals from agricultural and land use activities.

Scope 3 Compliance: As per 2026 requirements, this report aims for at least 95% coverage for Scope 3 reporting. This means accounting for and reporting at least 95% of total required Scope 3 emissions, with any exclusions not exceeding 5%. This ensures a comprehensive and transparent assessment of value chain impacts.

2. Map Lifecycle (LCI Inventory Stages)

The lifecycle of vistydftvv is mapped into five key stages, consistent with a cradle-to-grave PCF approach, covering all material and energy flows relevant to the product\'s footprint.

Raw Material Extraction & Processing: Covers the sourcing and initial manufacturing of all components listed in the Detailed Bill of Materials (BOM).

Manufacturing: Encompasses the energy consumption and associated emissions during the assembly and production of vistydftvv at the sfugvuouri facility in China.

Transport: Includes both upstream transportation of raw materials to the manufacturing facility and downstream transportation of the finished product to the market in Europe, including last-mile delivery.

Use Phase: Accounts for the energy consumed by the product during its specified lifespan.

End-of-Life (EoL): Addresses the emissions or avoided emissions associated with the disposal, recycling, or recovery of the product at the end of its useful life.

3. Collect Data (Primary/Secondary Data Points)

Data collection involved a combination of primary data provided for vistydftvv and secondary, industry-standard emission factors.

Detailed Bill of Materials (BOM) for vistydftvv

The following detailed Bill of Materials (BOM) was used to calculate the material impact. Emission Factors are based on industry averages (e.g., Ecoinvent/DEFRA equivalents) for primary materials.

ID	Description	Category	Process	Qty (kg)	Emission Factor (kgCO2e/kg)	Total Carbon (kgCO2e)
M001	Plastic Casing	Polymer	Injection Molding	0.200	3.50	0.700
M002	PCB Board	Electronics	Manufacturing	0.050	15.00	0.750
M003	Copper Wiring	Metal	Extrusion	0.010	8.00	0.080
M004	Lithium-ion Battery	Battery	Manufacturing	0.100	20.00	2.000
M005	Packaging (Cardboard)	Paper/Wood	Pulping & Forming	0.150	1.00	0.150

Logistics Data

Upstream Transport Mode: Road Freight (HGV > 16t)

Upstream Transport Distance: 1500 km (average for European supply chain to China)

Downstream Transport Mode: Road Freight (HGV > 16t) for primary distribution, followed by Van Delivery for last-mile.

Downstream Transport Distance: 200 km (primary distribution in Europe)

Last-Mile Delivery Channel: Van Delivery (estimated 50 km)

Energy Customization Data (Manufacturing Phase)

Renewable Energy Usage: 50%

Energy Intensity (kWh/unit): 15 kWh/unit

Assumed Grid Emission Factor (China): 0.58 kgCO2e/kWh (Based on IEA 2021: 0.6093 kgCO2/kWh and MEE 2021: 0.5568 kg CO2/kWh, average used for illustrative purposes).

Product Use Phase Data

Product Lifespan: 5 years

Energy Consumption in Use: 10 kWh/year

Assumed European Grid Emission Factor (Use Phase): 0.25 kgCO2e/kWh (Illustrative average for Europe)

End-of-Life (EoL) Scenarios

Recyclability Percentage: 70%

Circular/Take-back Programs: Yes, via established take-back scheme

Assumed EoL Factors:

Landfill/Incineration (non-recyclable): 0.1 kgCO2e/kg (for material disposed)

Recycling Credit (recyclable): -0.5 kgCO2e/kg (for material recycled, representing avoided virgin material production)

4. Calculate Emissions (Activity * Emission Factor = CO2e)

Emissions are calculated for each lifecycle stage and categorized according to the GHG Protocol Scopes. A comprehensive Scope 3 assessment is performed to ensure over 95% coverage, reflecting the upstream and downstream value chain activities. All calculations are in kgCO2e.

GHG Protocol Scope Definitions:

Scope 1: Direct GHG Emissions from sources owned or controlled by the company (e.g., combustion in owned boilers, vehicles).

Scope 2: Indirect GHG Emissions from Purchased Energy (e.g., electricity, heat, steam).

Scope 3: Other Indirect GHG Emissions occurring from sources not owned or controlled by the company but related to its value chain (e.g., purchased goods, transport, use of sold products, end-of-life).

Emissions Breakdown by Lifecycle Stage and Scope

1. Raw Material Extraction & Processing (Scope 3, Category 1)

This stage accounts for the emissions embedded in the purchased raw materials and components, derived directly from the provided BOM data.

Description	Qty (kg)	Emission Factor (kgCO2e/kg)	Total CO2e (kg)
Plastic Casing	0.200	3.50	0.700
PCB Board	0.050	15.00	0.750
Copper Wiring	0.010	8.00	0.080
Lithium-ion Battery	0.100	20.00	2.000
Packaging (Cardboard)	0.150	1.00	0.150

2. Manufacturing (Scope 2)

Emissions from the manufacturing process are primarily from purchased electricity, adjusted for renewable energy usage at the China-based facility.

Total Energy Consumed: 15 kWh/unit

Renewable Energy Share: 50%

Non-renewable Energy Consumed: 15 kWh * (1 - 0.50) = 7.5 kWh/unit

China Grid Emission Factor: 0.58 kgCO2e/kWh

Manufacturing Emissions (Scope 2): 7.5 kWh/unit * 0.58 kgCO2e/kWh = 4.350 kgCO2e/unit

Scope 1 Emissions: Not applicable with provided data (assuming no direct combustion or company-owned vehicles at factory gate).

Total Scope 2 Emissions: 4.350 kgCO2e

3. Transport (Scope 3, Categories 4 & 9)

Calculations include both upstream (raw material delivery) and downstream (finished product distribution) transportation.

Product Weight (from BOM): 0.510 kg/unit

Upstream Transport (Raw Materials - Scope 3, Category 4)

Transport Mode: Road Freight (HGV > 16t)

Transport Distance: 1500 km

Emission Factor (Road Freight): 0.062 kgCO2e/tonne-km (equivalent to 0.000062 kgCO2e/kg-km)

Upstream Emissions: (0.510 kg * 1500 km) * 0.000062 kgCO2e/kg-km = 0.047 kgCO2e

Downstream Transport (Finished Product - Scope 3, Category 9)

Primary Distribution:

Transport Mode: Road Freight (HGV > 16t)

Transport Distance: 200 km

Emission Factor (Road Freight): 0.062 kgCO2e/tonne-km

Emissions: (0.510 kg * 200 km) * 0.000062 kgCO2e/kg-km = 0.006 kgCO2e

Last-Mile Delivery:

Transport Mode: Van Delivery

Transport Distance: 50 km (estimated)

Emission Factor (Van Delivery): 0.25 kgCO2e/km

Emissions: 50 km * 0.25 kgCO2e/km = 12.500 kgCO2e

Total Scope 3 (Categories 4 & 9) Emissions: (0.047 + 0.006 + 12.500) = 12.553 kgCO2e

4. Use Phase (Scope 3, Category 11)

Emissions from product use over its lifespan based on energy consumption.

Product Lifespan: 5 years

Energy Consumption in Use: 10 kWh/year

Total Energy Consumption over Lifespan: 10 kWh/year * 5 years = 50 kWh/unit

Assumed European Grid Emission Factor: 0.25 kgCO2e/kWh

Use Phase Emissions: 50 kWh/unit * 0.25 kgCO2e/kWh = 12.500 kgCO2e

Total Scope 3 (Category 11) Emissions: 12.500 kgCO2e

5. End-of-Life (EoL) (Scope 3, Category 12)

Emissions and avoided emissions from disposal and recycling scenarios.

Total Product Weight: 0.510 kg/unit

Recyclable Portion: 70% * 0.510 kg = 0.357 kg

Non-Recyclable Portion: 30% * 0.510 kg = 0.153 kg

Recycling Credit: -0.5 kgCO2e/kg

Landfill/Incineration Factor: 0.1 kgCO2e/kg

Emissions from Recycling: 0.357 kg * -0.5 kgCO2e/kg = -0.179 kgCO2e

Emissions from Disposal: 0.153 kg * 0.1 kgCO2e/kg = 0.015 kgCO2e

Net EoL Emissions: -0.179 + 0.015 = -0.164 kgCO2e

Total Scope 3 (Category 12) Emissions: -0.164 kgCO2e

Overall Product Carbon Footprint (PCF) for vistydftvv

The total Product Carbon Footprint for one functional unit of vistydftvv is summarized below:

Lifecycle Stage	GHG Scope	Total CO2e (kg)
Raw Material Extraction & Processing	Scope 3 (Category 1)	3.680
Manufacturing	Scope 2	4.350
Upstream Transport (Raw Materials)	Scope 3 (Category 4)	0.047
Downstream Transport (Primary & Last-Mile)	Scope 3 (Category 9)	12.506
Use Phase	Scope 3 (Category 11)	12.500
End-of-Life Treatment	Scope 3 (Category 12)	-0.164

Summary of Emissions by GHG Protocol Scope

GHG Scope	Total CO2e (kg)
Scope 1	0.000 (Not applicable with provided data)
Scope 2	4.350
Scope 3	28.569

5. Review & Report

Hotspots Analysis

The PCF analysis reveals the following key emission hotspots for vistydftvv:

Downstream Transport (Last-Mile Delivery): This stage contributes significantly (approx. 38% of total PCF), largely due to the relatively high emission factor associated with van delivery over a significant distance for a single unit. Optimizing last-mile logistics or exploring greener delivery options could yield substantial reductions.

Use Phase: The energy consumption during the product\'s 5-year lifespan is another major contributor (approx. 38%). Improving energy efficiency of the product or encouraging the use of renewable energy sources by consumers would be critical.

Manufacturing (Scope 2): Although 50% renewable energy is used, the remaining grid electricity in China still represents a notable portion (approx. 13%) of the footprint. Increasing renewable energy procurement or investing in on-site renewables at the manufacturing facility would be impactful.

Raw Materials: The raw materials, particularly the Lithium-ion Battery and PCB Board, contribute significantly to the upstream footprint (approx. 11%). Material substitution with lower-impact alternatives or working with suppliers on decarbonization efforts would be beneficial.

Reliability and Limitations

The reliability of this PCF analysis is contingent on several factors:

Data Quality: While primary data for BOM, energy usage, and EoL scenarios were provided, secondary emission factors (e.g., for materials, transport modes, grid electricity) were used, which are based on industry averages (e.g., Ecoinvent, DEFRA). These are approximations and actual emissions may vary based on specific supplier data.

System Boundary: The "factory_gate" system boundary for direct operations combined with a comprehensive Scope 3 assessment provides a broad view, but detailed impacts beyond direct control (e.g., specific manufacturing processes of raw material suppliers) rely on generic data.

Assumptions: Several assumptions were made for placeholder values (e.g., transport distances, specific emission factors for EoL processes, European grid mix for use phase) due to the nature of the prompt. Refinement with actual operational data would enhance accuracy.

2026 LSR Standard: While the LSR Standard is acknowledged, a detailed quantification of land use and carbon removals was not performed due to the absence of specific land-related activity data for the product\'s value chain. The standard takes effect from January 1, 2027.

Scope 3 Coverage: The report aims for 95% Scope 3 coverage, as required by 2026 updates, by considering all relevant upstream and downstream categories. However, the granularity of data for all sub-categories might still be an area for further refinement.

Recommendations for Reduction

Logistics Optimization: Investigate more efficient last-mile delivery methods (e.g., electric vehicles, optimized routing, local hubs) and explore multimodal transport for longer distances to reduce transport emissions.

Energy Efficiency & Renewables: Implement further energy efficiency measures in the product design to reduce use-phase consumption. Increase the share of renewable energy in manufacturing operations, potentially through Power Purchase Agreements (PPAs) or on-site generation.

Sustainable Sourcing: Engage with raw material suppliers to obtain primary emission data and identify opportunities for sourcing lower-carbon materials or components. Focus on high-impact items like batteries and PCBs.

Circular Economy Strategies: Strengthen take-back programs and explore product-as-a-service models to extend product lifespan and ensure effective recycling or repurposing of components.

Data Improvement: Continuously improve data collection for Scope 3 emissions by engaging deeper with supply chain partners to gather primary data, moving away from average emission factors where possible.

Confidential - Internal Use Only |